| **Sl. No.** | **Existing clause** | **Queries asked by the bidder** | **POWERGRID’s clarification** |
| --- | --- | --- | --- |
| **1** | Volume II, Section 1 A, Clause 1.6, Point 4ii), 5 ii) & 6 ii),

|  |  |
| --- | --- |
| 4  | Sag-Tensions under Condition-I(LILO portion at NP Kunta end)-one circuit of D/C Line |
| ii) | Sag for ruling spanat minimum temp (0 deg C) and no windcondition (m) | ≥9.67 |
|  | Sag-Tensions under Condition- II (S/C Line) S/C portion between tapping point of 400kV Cuddapah-Somnahalli line LILOed at NP Kunta & Kolar. |
| ii) | Sag for ruling spanat minimum temp (0deg C) and no windcondition (m) | ≥9.67 |
|  | Sag-Tensions under Condition-III (LILO portion at Kolar end) -one circuit of D/C Line |
| ii) | Sag for ruling spanat minimum temp (0deg C) and no windcondition (m) | ≥9.67 |

 | We requesting you to kindly modify as follow:4 Sag-Tensions under Condition-I (LILO portion atNP Kunta end)- one circuit of D/C Lineii) Sag for ruling span at minimum temp (0 deg C) andno wind condition (m) : ≥ 9.005 Sag-Tensions under Condition-II (S/C Line) S/Cportion between tapping point of 400kV Cuddapah-Somnahalli line LILOed at NP Kunta & Kolar.ii) Sag for ruling span at minimum temp (0 deg C) andno wind condition (m) : ≥ 9.006 Sag-Tensions under Condition-III (LILO portionat Kolar end) - one circuit of D/C Line.ii) Sag for ruling span at minimum temp (0 deg C) andno wind condition (m) : ≥ 9.00 | No change in provisions of TS is envisaged. |