|  |  |  |  |
| --- | --- | --- | --- |
| S. N | Clause No. | Existing clause | Corrected clause |
| 1. | Specification: Volume-II, Part 4, Section VII, Cl. No. 1.3 | The HTLS conductor shall meet the following minimum requirements:  Overall diameter of complete conductor Not exceeding 28.62mm and  Not less than 21 mm | The HTLS conductor shall meet the following minimum requirements:  Overall diameter of complete conductor Not exceeding 28.62mm and  Not less **than 25 mm** |