| **Sl. No.** | **Clause Reference** | **Existing Provision** | **Amended Provision** |
| --- | --- | --- | --- |
| 1 | Volume II, Section I, Clause 3, Sl. No. C 4 ii) |

|  |  |
| --- | --- |
| Sag for ruling span at minimum temp ( 0 deg C) and no wind condition (m) | ≥9.663 |

 |

|  |  |
| --- | --- |
| Sag for ruling span at minimum temp **( 2.5 deg C)** and no wind condition (m) | **≥9.65** |

 |
| 2 | Volume II, Section I, Clause 3, Sl. No. C 4 iv) |

|  |  |
| --- | --- |
| Tension at 0°C and 2/3 wind condition(32 kg/m2 wind pressure) | ≤ 4523 kg & not exceeding 70% of UTS of proposed conductor |

 |

|  |  |
| --- | --- |
| Tension at **2.5°C** and 2/3 wind condition(32 kg/m2 wind pressure) | **≤ 4474 kg** & not exceeding 70% of UTS of proposed conductor |

 |
| 3 | Volume II, Section I, Clause 13,  | **Service Condition**………………..

|  |  |
| --- | --- |
| Minimum ambient temperature (Degree Celsius)  | 0 |

……………………………. | **Service Condition**………………..

|  |  |
| --- | --- |
| Minimum ambient temperature (Degree Celsius)  | **2.5** |

……………………………. |