**Corrigendum to Technical QR**

|  |  |  |  |
| --- | --- | --- | --- |
| **SN** | **Clause No. / Section of Tender****Document** | **Existing Provision in Tender** | **Modified provision** |
| 1 | Annexure-A (BDS)-QR 1.0 TechnicalExperience 1.1(a)  | The bidder must have designed, manufactured, type tested and supplied cumulatively atleast 24 (Twenty-Four) km of single core, 66kV/33kV/11kV or higher grade XLPE insulated cable which must have been in satisfactory# operation for at least 2 (two) years as on the originally scheduled date of bid opening i.e.08/10/2025 | The bidder must have designed, manufactured, type tested and supplied cumulatively at least 24 (Twenty-Four) km of **single core or Three Core**, 66kV/33kV/11kV or higher grade XLPE insulated cable which must have been in satisfactory# operation for at least 2 (two) years as on the originally scheduled date of bid opening i.e. 08/10/2025. |
| 2. | Annexure-A (BDS)-QR 1.0 TechnicalExperience 1.2  | The bidder must have successfully executed a contract which includes underground laying & termination in a single contract, at least 24 (Twenty Four) km of single core, 11kV or higher grade XLPE insulated cable including testing and commissioning which should must have been in satisfactory operation for at least 2 (two) years as on the originally scheduled date of bid opening mentioned above.  | The bidder must have successfully executed a contract which includes underground Laying & termination in a single contract, at least 24 (Twenty-Four) km of **single core or Three Core**, 11kV or higher grade XLPE insulated cable including testing and commissioning which must have been in satisfactory# operation for at least 2 (two) years as on the originally scheduled date of bid opening. |